


	SECTION 095416 / SECTION 09 54 16
LUMINOUS CEILINGS
Translucents™ Canopies with physical hanging and attachment devices for     suspending

	
	Product Specification


GENERAL
RELATED DOCUMENTS
Drawings and general provisions of the Contract, including General and Supplementary Conditions and Division 1 Specification Sections, apply to this Section.
REFERENCES
ASTM E1264 and as tested in accordance with ASTM E84
Class A requirements of NFPA 286 and IBC (UBC) as interior finishes, not to be part of an air supply/return system
NFPA 13 and their local codes for guidance where automatic fire detection and suppression systems are present
SUMMARY
This Section includes, but is not limited to, the following:
Ceiling Canopies
Physical hanging and attachment devices
Related Sections include the following:
Division 90 20 00 (9) – Section 09 21 16 – Gypsum Board Assemblies
Division 09 50 00 Ceilings
Division 23 00 00 (15) Heating, Ventilating, and Air Conditioning (HVAC)
Division 26 00 00 (16) Electrical
SUBMITTALS
Samples: Submit manufacture’s samples and technical data for review. 
Shop Drawings:
Reflected ceiling plans: Submit canopy layout indicating dimensions, lighting fixture locations, and related mechanical components.
Assembly drawings: Indicate installation details, accessory attachments and installation of related components.
Manufacturer’s Data:
System Details: Submit manufacturer’s catalog cuts or standard drawing showing details of system with project conditions clearly identified and manufacturer’s recommended installation instructions.
Maintenance Data: For finishes to include in maintenance manuals.
DELIVERY, STORAGE, AND HANDLING
Deliver canopy, suspension system components, and accessories to Project site in original, unopened packages and store them in a fully enclosed, conditioned space where they will be protected against damage from moisture, humidity, temperature extremes, direct sunlight, surface contamination, and other causes. 
Inspection: Promptly inspect delivered materials; file freight claims for damage during shipment, and/or replacement materials, as required.
Storage: Store in manner that will prevent warpage, scratches, or damage of any kind. Prevent interference to/by other trades and any other adverse job conditions due to storage locations or methods.
Handling: Handle in such a manner as to ensure against racking, distortion, or physical damage of any kind.
QUALITY ASSURANCE
Source Limitations for Canopies: Obtain each set of canopy with hanging and attachment devices for suspending from one source with resources to provide products of consistent quality in appearance, physical properties, and performance.
Fire-Test-Response Characteristics: Provide luminous panels with surface-burning characteristics complying with ASTM E 1264 for Class A materials as determined by testing identical products per ASTM E 84 by UL or another testing and inspecting agency acceptable to authorities having jurisdiction.
Seismic Standard: For installations on projects designated seismic design categories   C-F, suspension wires that are a minimum of no. 12 gauge galvanized, soft-annealed, mild steel wire shall be used.
Please refer to USG Seismic Technical Guide - Specialty and Decorative Ceilings SC2494 for more information about the seismic guidelines for specialty and decorative ceilings. Because codes continue to evolve, check with a local official prior to designing and installing a ceiling system. Other restrictions and exemptions may apply.
Pre-installation Conference: Conduct conference at Project site to comply with requirements in Division 1 Section “Project Management and Coordination.”Installer Qualifications: An experienced installer who has completed metal pan ceiling systems similar in material, design, and extent to those indicated for this Project and whose work has resulted in construction with a record of successful in-service performance.
Source quality control: Manufacturer will provide test certification for ceiling system as required complying with industry performance standards specified by various agencies.
Pre-installation Conference: Conduct conference at Project site to comply with requirements in Division 1 Section "Project Meetings."
PROJECT CONDITIONS
Environmental Limitations: Do not install decorative grid and wire-grate panels until spaces are enclosed and weather-proof, wet work in spaces is complete and dry, work above ceilings is complete and ambient temperature and humidity conditions are maintained at the levels indicated for Project when occupied for its intended use.
PRODUCTS AND MANUFACTURERS
MANUFACTURER
All manufactured by USG (United States Gypsum Company, USG Interiors), Chicago, IL, USA, in compliance with applicable ASTM Standards. www.usgdesignstudio.com

MATERIALS
A. Basis of Design: TRANSLUCENTS™ Canopies 2’ x 6’ (actual 24"x 72" ± 2") with installation hardware to hang the canopy panels. See Finish Schedule for Design Selections.  Luminous Ceilings: LC
1. LC-1: Wave Kit, Model No: TRNWAV2465, Formed Panel Dimension: 12"H x 23.38"W x 65" L: Part Number 747_ _ _ 
2. LC-2: Vault or Valley Kit, Model No. TRNVLT/VLY2468, Formed Panel Dimension: 9"H x 23.38"W x 68" L: Part Number 747_ _ _
3. LC-3: Vault Only Kit, Model No. TRNVLT2468, Formed Panel Dimension: 9"H x 23.38"W x 68" L: Part Number 747_ _ _
4. LC-4: Valley Only Kit, Model No. TRNVLY2468, Formed Panel Dimension: 9"H x 23.38"W x 68" L: Part Number 747_ _ _
0. Spec. Note, Optional canopy types are as follows, unless otherwise indicated: 
a. Woven, Shimmer, Textiles, Natural, Industrial
b. Embossed Acrylic. 
EXECUTION
EXAMINATION
Examine substrates, areas, and conditions, including structural framing to which grid or panels attach or abut, with Installer present, for compliance with requirements specified in this and other Sections that affect ceiling installation and anchorage and with requirements for installation tolerances and other conditions affecting performance of acoustical panel ceilings.
Proceed with installation only after unsatisfactory conditions have been corrected.
PREPARATION
Measure each ceiling area and establish layout of canopies and comply with layout shown on reflected ceiling plans.
INSTALLATION
General: Install canopies to comply with manufacturer’s current “Design and Installation Guide” IC594 written instructions and seismic requirements indicated.
Drawing reference: Install in accordance with approved shop drawings and locate canopies in accordance with location dimensions relative to elevations.
CLEANING
Clean exposed surfaces of canopies, including trim and edge moldings after removing strippable, temporary protective covering, if any. Comply with manufacturer’s written instructions for stripping of temporary protective covering, cleaning, and touchup of minor finish damage. Remove and replace canopy components that cannot be successfully cleaned and repaired to permanently eliminate evidence of damage, including dented and bent units.

Safety First!
Follow good safety and industrial hygiene practices during handling and installing of all products and systems. Take necessary precautions and wear the appropriate personal protective equipment as needed. Read material safety data sheets and related literature on products before specification and/or installation.

END OF SECTION 09580
**************************************************************************
The text material contained herein is intended for use as product reference material by architects, engineers, other design professionals, contractors, building code officials, or other competent construction industry trade factors having an interest in the selection, specification and use of products manufactured by the subsidiaries of USG Corporation. It is intended solely as technical support incident to the sale and use of our products.
These materials may be printed and/or transferred electronically as needed by the user. Modification of this information is the sole responsibility of the Design Professional. Any unauthorized duplication or reuse of the material contained herein is a violation of law.
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